[bookmark: OLE_LINK1][bookmark: OLE_LINK2]Model and specification of combined orthopedic external fixation bracket
	model
	Part name
	Part model
	material quality
	Component specifications（mm）
	number

	

WJZⅠ-01A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	[bookmark: OLE_LINK19][bookmark: OLE_LINK20](Φ3.0~Φ5.5, interval0.5）×（50～200，interval5）、Φ6.0×（80～300，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	(Φ5.0、Φ5.5）×（50～200，interval5）、Φ6.0×（80～300，interval5）
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ2.0、Φ2.5、3.0、3.5）/(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）
	2

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	



WJZⅠ-02A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ3.0~Φ5.5,interval0.5）×（50～200，interval5）、Φ6.0×（80～300，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	(Φ5.0、Φ5.5）×（50～200，interval5）、Φ6.0×（80～300，interval5）
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ2.0、Φ2.5、3.0、3.5）/(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）
	2

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0~Φ6.0,interval0.5）/(Φ3.0~Φ6.0,interval0.5）
	1

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	

WJZⅠ-03A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ3.0~Φ5.5,interval0.5）×（50～200，interval5）、Φ6.0×（80～300，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	(Φ5.0、Φ5.5）×（50～200，interval5）、Φ6.0×（80～300，interval5）
	

	
	Nail bar clamp
	WJZJ02A(B)
	Sc/T
	(Φ2.0、Φ2.5、3.0、3.5）/(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）
	2

	
WJZⅠ-04A(B)
	Joint connector
	WJZG01/02/03 A(B)
	Sc/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/（50～250，interval5）
	1

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ2.0、Φ2.5、Φ3.0）/(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）
(Φ3.5）/(Φ3.5、Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）
	
4

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	WJZⅠ-05A(B)
	Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ5.0、Φ6.0）×（50～200，interval5）、Φ8.0×（100～200，interval5）
	2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	



1
	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ5.0/Φ5.0、Φ6.0/Φ6.0、Φ8.0/Φ8.0
	4

	
	Rod clamp
	WJZB02/03A(B)
	Sc/T
	Φ5.0/Φ5.0、Φ6.0/Φ6.0、Φ8.0/Φ8.0
	4

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ2.0、Φ2.5、Φ3.0、Φ3.5、Φ4.0）/(Φ5.0、Φ6.0、Φ8.0）
	2

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ5.0、Φ6.0、Φ8.0）×（50～200，interval5）
	4

	



WJZⅠ-06A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEKT
	
(Φ5.0、Φ6.0）×（50～200，interval5）、Φ8.0×（100～200，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ5.0/Φ5.0、Φ6.0/Φ6.0、Φ8.0/Φ8.0
	1

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0、Φ6.0、Φ8.0）
	4

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	



WJZⅡ-01A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	1

	
	Clip block
	WJZD02A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	1

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ5.0~Φ8.0，interval0.5）×（50～200，interval5）
	1

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ5.0~Φ8.0，interval0.5）/(Φ5.0~Φ8.0，interval0.5）
	2

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	

WJZⅡ-02A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	4

	
	
	WJZJ03/05A(B)
	Sc/T
	
	




2
	



WJZⅡ-03A(B)
	Connecting rod
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	Connecting pipe
	WJZK01/02A(B)
	Sc/T
	(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	2

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	2

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ5.0~Φ8.0，interval0.5）/(Φ5.0~Φ8.0，interval0.5）
	2

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	2

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ5.0~Φ8.0，interval0.5）×（50～200，interval5）
	2

	



WJZⅡ-04A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	2

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ5.0~Φ8.0，interval0.5）/(Φ5.0~Φ8.0，interval0.5）
	4

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ5.0~Φ8.0，interval0.5）×（50～200，interval5）
	4

	




WJZⅡ-05A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS05A(B)
	Sc/AL/Cf/PEEK/T
	(Φ5.0~Φ8.0，interval0.5）×（80～300，interval5）
	1

	
	
	WJZK05A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0）/(Φ5.0~Φ8.0，interval0.5）
	3

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ5.0~Φ8.0，interval0.5）/(Φ5.0~Φ8.0，interval0.5）
	2

	
	
	WJZB02/03A(B)
	Sc/T
	
	



3
	


WJZⅡ-06A(B)
	Connecting rod
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	Connecting pipe
	WJZK01/02A(B)
	Sc/T
	(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	3

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	3

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	5

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	



WJZⅡ-07A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	2

	
	
	WJZB02/03(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	2

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（50～200，interval5）
	2

	
WJZⅡ-08A(B)
	Joint connector
	WJZG01/02/03 A(B)
	Sc/T
	(Φ6.5、Φ7.0、Φ7.5、Φ8.0）/（150～400，interval5）
	1

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ6.5、Φ7.0、Φ7.5、
Φ8.0）
	4

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	

WJZⅡ-09A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	4

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
WJZⅡ-10A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	


4
	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	2

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	2

	
	pillar
	WJZZ02A(B)
	Sc/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（50～200，interval5）
	2

	


WJZⅡ-11A(B)
	Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	Connecting rod / pipe
	WJZK01/02A(B)
	Sc/T
	(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	6

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	2

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	


WJZⅡ-12A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	4

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	1

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	



WJZⅡ-13A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	2

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	4

	
	
	WJZB02/03A(B)
	Sc/T
	
	


5

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	1

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（50～200，interval5）
	2

	






WJZⅡ-14A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（140～300，interval5）
	1

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	3

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	4

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	1

	
	pillar
	WJZZ01/02A(B)
	Sc/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（50～200，interval5）
	2

	






WJZⅡ-15A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（140～300，interval5）
	1

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS04A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（140～300，interval5）
	1

	
	
	WJZK04A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	3

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	5

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	WJZⅡ-16
	Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	1



6
	A(B)
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（140～300，interval5）
	2

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Adjusting lever
	WJZT01A(B)
	Sc/Sc+AL/T
	(Φ7.0、Φ7.5、Φ8.0）×（200～400，interval5）
	2

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	6

	
	
	WJZB02/03A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	6

	
	
	WJZJ03/05A(B)
	Sc/T
	
	

	
WJZⅡ-17A(B)
	Adjusting lever
	WJZT02A(B)
	Sc/T
	(Φ7.0、Φ7.5、Φ8.0）×（200～400，interval5）
	1

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	2

	
	
	WJZJ03A(B)
	Sc/T
	
	

	
WJZⅡ-18A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～400，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ02A(B)
	Sc/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	2

	



WJZⅡ-19A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ7.0、Φ7.5、Φ8.0）×（80～200，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	1

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	1

	
	
	WJZJ03A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	1

	
	
	WJZB02A(B)
	Sc/T
	
	

	WJZⅡ-20
	Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ7.0、Φ7.5、Φ8.0）×（80～200，interval5）
	3
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	A(B)
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ7.0/Φ7.0、Φ7.5/Φ7.5、Φ8.0/Φ8.0
	2
	

	
	
	WJZB02/03 A(B)
	Sc/T
	
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ7.0、Φ7.5、Φ8.0）
	2
	

	
	
	WJZJ03/05 A(B)
	Sc/T
	
	
	

	
	Nail bar clamp
	WJZJ04A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ3.0、Φ3.5、Φ4.0、Φ4.5、Φ5.0）/(Φ5.0、Φ5.5、Φ6.0、
Φ6.5、Φ7.0、Φ7.5、Φ8.0）
	1
	

	











WJZⅡ-21A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1
	

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	2
	

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1
	

	
	Standard Taylor rod
	WJZW01A(B)
	Sc/AL/T
	L50～L300，interval5
	1
	

	
	Quick mount Taylor bar
	WJZW02A(B)
	Sc/AL/T
	L50～L300，interval5
	2
	

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval5
	1
	

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval5
	4
	

	
	Offset slot needle base
	WJZL07A(B)
	Sc/AL/T
	L10～L150，interval5
	1
	

	
	Universal joint
	WJZL08A(B)
	Sc/AL/T
	L20，L25，L30，L35，L40，L45，L50
	6
	

	
	Porous connecting piece
	WJZL13A(B)
	Sc/AL/T
	L20～L200，interval1
	2
	

	
	Arc connecting piece
	WJZL14A(B)
	Sc/AL/T
	L50～L350，interval5
	2
	

	
	Threaded column
	WJZL18A(B)
	Sc/AL/T
	L10～L150，interval5
	1
	

	
	Nut column
	WJZL17A(B)
	Sc/AL/T
	L10～L150，interval5
	1
	

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval5
	2
	

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval5
	2
	

	
	bushing
	WJZL22A(B)
	AL/T
	L10，L15，L20，L25，L30，L35，L40，L45，L50
	6
	

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L15，L20，L25，L30，L35，L40
	2
	

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval5
	25
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	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	46

	
	[bookmark: OLE_LINK63][bookmark: OLE_LINK64]Nut
	WJZL26A(B)
	Sc/AL/T
	L5，L10，L15，L20
	46

	
	earring
	WJZL30A(B)
	Sc/AL/T
	L10～L100，interval5
	5

	
	Ball bowl gasket
	WJZL40A(B)
	Sc/AL/T
	L5，L10，L15，L20
	1

	
	Marking card
	WJZL41A(B)
	AL/T
	L=10
	3

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	












WJZⅡ-22A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	3-lug 2/3-ring
	WJZH02A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/3 ring
	WJZH08A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Bending bar
	WJZL02A(B)
	Sc/AL/T
	L50～L350，interval5
	1

	
	Diagonal brace
	WJZL03A(B)
	Sc/AL/T
	L50～L350，interval5
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval5
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval5
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L20，L25，L30，L35，L40，L45，L50
	2

	
	90 ° conversion block
	WJZL11A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	90 ° conversion plate
	WJZL12A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	90 ° connecting piece
	WJZL15A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Pitted nut
	WJZL20A(B)
	Sc/AL/T
	L10，L15，L20，L25，L30，L35，L40，L45，L50
	2

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L10，L15，L20，L25，L30，L35，L40，L45，L50
	6

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval5
	4
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	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	44

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5，L10，L15，L20
	44

	
	spring
	WJZL27A(B)
	Sc/T
	L15～L100，interval5
	1

	
	Indenter
	WJZL28A(B)
	Sc/AL/T
	L15，L20，L25，L30，L35，L40，L45，L50
	1

	
	control
	WJZL29A(B)
	Sc/AL/T
	L15～L100，interval5
	1

	
	Quadrangular curved column
	WJZL31A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Adjustable universal hinge
	WJZL32A(B)
	Sc/AL/T
	L10～L200，interval5
	1

	
	Conversion chip
	WJZL33A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Single hole connecting piece
	WJZL34A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Kirschner wire guide block
	WJZL35A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Steering needle base
	WJZL37A(B)
	Sc/AL/T
	L10～L200，interval5
	1

	
	Universal rail connecting piece
	WJZL38A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Ring needle connecting rod
	WJZL39A(B)
	Sc/AL/T
	L10～L300，interval5
	1

	
	Ball bowl gasket
	WJZL40A(B)
	Sc/AL/T
	L5，L10，L15，L20
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	





WJZⅡ-23A(B)
	Four lug half ring
	WJZH03A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Unidirectional extender
	WJZL01A(B)
	Sc/AL/T
	L50～L300，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Universal joint
	WJZL08A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L5～L400，interval2
	1
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	[bookmark: OLE_LINK105][bookmark: OLE_LINK106]screw threadUnidirectional joint
	WJZL10A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	Porous connecting piece
	WJZL13A(B)
	Sc/AL/T
	L20～L200，interval1
	1

	
	Track connecting piece
	WJZL16A(B)
	Sc/AL/T
	L20～L100，interval2
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Pitted bolt
	WJZL20A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	27

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	49

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	49

	
	spring
	WJZL27A(B)
	Sc/T
	L15～L100，interval2
	1

	
	earring
	WJZL30A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Connecting piece
	WJZL36A(B)
	Sc/AL/T
	L40～L200，interval2
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	





WJZⅡ-24A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/3 ring
	WJZH08A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Unidirectional extender
	WJZL01A(B)
	Sc/AL/T
	L50～L300，interval2
	1

	
	Bending bar
	WJZL02A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	90 ° conversion block
	WJZL11A(B)
	Sc/AL/T
	L10～L100，interval2
	1
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	90 ° conversion plate
	WJZL12A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	90 ° connecting piece
	WJZL15A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Track connecting piece
	WJZL16A(B)
	Sc/AL/T
	L20～L100，interval2
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	2

	
	Pitted nut
	WJZL20A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	35

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	50

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	50

	
	spring
	WJZL27A(B)
	Sc/T
	L15～L100，interval2
	1

	
	Indenter
	WJZL28A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	control
	WJZL29A(B)
	Sc/AL/T
	L15～L100，interval2
	1

	
	Quadrangular curved column
	WJZL31A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Adjustable universal hinge
	WJZL32A(B)
	Sc/AL/T
	L10～L200，interval2
	1

	
	Conversion chip
	WJZL33A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Single hole connecting piece
	WJZL34A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Steering needle base
	WJZL37A(B)
	Sc/AL/T
	L10～L200，interval2
	1

	
	Universal rail connecting piece
	WJZL38A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	

WJZⅡ-25A(B)
	3-lug 2/3-ring
	WJZH02A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Four lug half ring
	WJZH03A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Standard Taylor rod
	WJZW01A(B)
	Sc/AL/T
	L50～L300，interval5
	1
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	Quick mount Taylor bar
	WJZW02A(B)
	Sc/AL/T
	L50～L300，interval5
	2

	
	Diagonal brace
	WJZL03A(B)
	Sc/AL/T
	L50～L350，interval5
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval5
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval5
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Offset slot needle base
	WJZL07A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Universal joint
	WJZL08A(B)
	Sc/AL/T
	L20，L25，L30，L35，L40，L45，L50
	6

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L20，L25，L30，L35，L40，L45，L50
	2

	
	screw thread Unidirectional joint
	WJZL10A(B)
	Sc/AL/T
	L20，L25，L30，L35，L40，L45，L50
	1

	
	Porous connecting piece
	WJZL13A(B)
	Sc/AL/T
	L20～L200，interval1
	1

	
	Arc connecting piece
	WJZL14A(B)
	Sc/AL/T
	L50～L350，interval5
	2

	
	Threaded column
	WJZL18A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Nut column
	WJZL17A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval5
	2

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L10，L15，L20，L25，L30，L35，L40，L45，L50
	6

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L15，L20，L25，L30，L35，L40
	2

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval5
	4

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	21

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5，L10，L15，L20
	21

	
	control
	WJZL29A(B)
	Sc/AL/T
	L15～L100，interval5
	1

	
	earring
	WJZL30A(B)
	Sc/AL/T
	L10～L100，interval5
	3

	
	Ring needle connecting rod
	WJZL39A(B)
	Sc/AL/T
	L10～L300，interval5
	1

	
	Ball bowl gasket
	WJZL40A(B)
	Sc/AL/T
	L5，L10，L15，L20
	1

	
	Marking card
	WJZL41A(B)
	AL/T
	L=10
	3
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	Kirschner wire guide block
	WJZL35A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	












WJZⅡ-26A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/3 ring
	WJZH08A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval5
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval5
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
	Threaded column
	WJZL18A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Nut column
	WJZL17A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval5
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L10，L15，L20，L25，L30，L35，L40，L45，L50
	6

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L15，L20，L25，L30，L35，L40
	2

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval5
	23

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	44

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5，L10，L15，L20
	44

	
	Connecting piece
	WJZL36A(B)
	Sc/AL/T
	L40～L200，interval5
	1

	
	Ball bowl gasket
	WJZL40A(B)
	Sc/AL/T
	L5，L10，L15，L20
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval5
	1

	
WJZⅢ-01A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～300，interval5）
	
3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、Φ9.5/Φ9.5、Φ10.0/Φ
	2
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	WJZB02/03 A(B)
	Sc/T
	10.0、Φ11.0/Φ11.0
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	3

	
	
	WJZJ03/05 A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ04A(B)
	Sc/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ5.0、Φ5.5、Φ6.0、
Φ6.5、Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）
	1

	



WJZⅢ-02A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	2

	
	
	WJZB02/03 A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	8

	
	
	WJZJ03/05 A(B)
	Sc/T
	
	

	






WJZⅢ-03A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～300，interval5）
	1

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS04A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～300，interval5）
	1

	
	
	WJZK04A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	3

	
	
	WJZB02/03 A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	8

	
	
	WJZJ03/05 A(B)
	Sc/T
	
	

	
WJZⅢ-04A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
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	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	1

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	5

	
	
	WJZB02/03 A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	1

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	2

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	





WJZⅢ-05A(B)
	Connecting rod
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	Connecting pipe
	WJZK01/02 A(B)
	Sc/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、Φ9.5/Φ9.5、Φ10/Φ10、Φ11/Φ11
	2

	
	
	WJZB02/03 A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8、Φ8.5、Φ9、Φ9.5、Φ10、Φ11）
	1

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11）×（50～200，interval5）
	2

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8、Φ8.5、Φ9、Φ9.5、Φ10、Φ11）
	2

	


WJZⅢ-06A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
4

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	6

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	2
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	pillar
	WJZZ01/02 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	2

	





WJZⅢ-07A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～200，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS04A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（200～400，interval5）
	2

	
	
	WJZK04A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	6

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	
	
	WJZJ03A(B)
	Sc/T
	
	

	
	Adjusting lever
	WJZT01A(B)
	Sc+AL/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（200～400，interval5）
	1

	



WJZⅢ-08A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～250，interval5）
	
6

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	6

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	
	
	WJZJ03A(B)
	Sc/T
	
	

	


WJZⅢ-09A(B)
	
Connecting rod / pipe
	WJZK01/02 A(B)
	Sc/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～250，interval5）
	
4

	
	
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
	

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	4

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
	4
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	WJZJ03A(B)
	Sc/T
	Φ9.5、Φ10.0、Φ11.0）
	

	




WJZⅢ-10A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	

3

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	6

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	2

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	4

	







WJZⅢ-11A(B)
	Connecting rod
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	Connecting pipe
	WJZK01/02 A(B)
	Sc/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～300，interval5）
	1

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	1

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	2

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	4

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	
	
	WJZJ03A(B)
	Sc/T
	
	

	
WJZⅢ-12A(B)
	

Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	

1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
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	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	
	
	WJZJ03A(B)
	Sc/T
	
	

	



WJZⅢ-13A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	4

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	2

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	2

	





WJZⅢ-14A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	

2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～300，interval5）
	1

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS04A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～350，interval5）
	1

	
	
	WJZK04A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB02A(B)
	Sc/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	3

	
	Nail bar clamp
	WJZJ02/03 A(B)
	Sc/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	7

	

WJZⅢ-15A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～300，interval5）
	2

	
	
	WJZK03/05/06 A(B)
	Sc/T
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	Adjusting lever
	WJZT01A(B)
	Sc+AL/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（200～400，interval5）
	2

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	6

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	6

	
	
	WJZJ03A(B)
	Sc/T
	
	

	

WJZⅢ-16A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
2

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	S/T
	
	

	
	Nail bar clamp
	WJZJ02A(B)
	Sc/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	
WJZⅢ-17A(B)
	Adjusting lever
	WJZT02A(B)
	Sc/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（200～400，interval5）
	1

	
	Nail bar clamp
	WJZJ03A(B)
	Sc/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	2

	




WJZⅢ-18A(B)
	Connecting rod
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～200，interval5）
	1

	
	
	WJZS02A(B)
	Sc/AL/ T
	
	

	
	Connecting pipe
	WJZK01/02 A(B)
	Sc/T
	Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～200，interval5）
	

	
	Clip block
	WJZD02A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	1

	
	Nail bar clamp
	WJZJ03A(B)
	Sc/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	1

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	1

	
	
	WJZB02A(B)
	Sc/T
	
	

	
WJZⅢ-19A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～300，interval5）
	
1

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Joint connector
	WJZG04A(B)
	Sc/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（200～700，间
	1
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	隔5）
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	1

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	4

	
	
	WJZJ02/03 A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	2

	
	
	WJZB02A(B)
	Sc/T
	
	

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	1

	







WJZⅢ-20A(B)
	
Connecting rod / pipe
	WJZS01A(B)
	Sc/AL/Cf/PEEK/T
	
(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（80～400，interval5）
	
4

	
	
	WJZS02A(B)
	Sc/AL/T
	
	

	
	
	WJZK01/02 A(B)
	Sc/T
	
	

	
	Connecting rod / pipe
	WJZS03/05/06 A(B)
	Sc/AL/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（150～300，interval5）
	2

	
	
	WJZK03/05/06 A(B)
	Sc/T
	
	

	
	Clip block
	WJZD01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	2

	
	pillar
	WJZZ01/02 A(B)
	Sc/Cf/PEEK/T
	(Φ8.0、Φ8.5、Φ9.0、Φ9.5、Φ10.0、Φ11.0）×（50～200，interval5）
	4

	
	Nail bar clamp
	WJZJ01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	(Φ4.0、Φ4.5、Φ5.0、Φ5.5、Φ6.0）/(Φ8.0、Φ8.5、Φ9.0、
Φ9.5、Φ10.0、Φ11.0）
	3

	
	
	WJZJ03A(B)
	Sc/T
	
	

	
	Rod clamp
	WJZB01A(B)
	(Sc+AL)/(Sc+Cf)/(PEEK+Sc)/T
	Φ8.0/Φ8.0、Φ8.5/Φ8.5、Φ9.0/Φ9.0、
Φ9.5/Φ9.5、Φ10.0/Φ10.0、Φ11.0/Φ11.0
	10

	
	
	WJZB02 A(B)
	Sc/T
	
	

	

WJZⅢ-21A(B)
	U-shaped foot ring
	WJZH04/05A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary U-shaped foot ring
	WJZH09/10A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/3 ring
	WJZH08A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4
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	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK T
	R40～R200，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	43

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	43

	
	Porous connecting piece
	WJZL13A(B)
	Sc/AL/T
	L20～L200，interval1
	2

	
	Connecting piece
	WJZL36A(B)
	Sc/AL/T
	L40～L200，interval2
	1

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	screw threadUnidirectional joint
	WJZL10A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	Track connecting piece
	WJZL16A(B)
	Sc/AL/T
	L20～L100，interval2
	1

	
	Indenter
	WJZL28A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	control
	WJZL29A(B)
	Sc/AL/T
	L15～L100，interval2
	1

	
	spring
	WJZL27A(B)
	Sc/T
	L15～L100，interval2
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	

WJZⅢ-22A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	2

	
	Four lug half ring
	WJZH03A(B)
	Sc/AL/Cf/PEEKT
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Standard Taylor rod
	WJZW01A(B)
	Sc/AL/T
	L50～L260，interval2
	6
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	Quick mount Taylor bar
	WJZW02A(B)
	Sc/AL/T
	L50～L260，interval2
	4

	
	Offset slot needle base
	WJZL07A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	2

	
	Threaded column
	WJZL18A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Bolt column
	WJZL17A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	46

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	46

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	46

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	Universal joint
	WJZL08A(B)
	Sc/AL/T
	L5～L400，interval2
	20

	
	Marking card
	WJZL41A(B)
	AL/T
	L5-L400，interval2
	10

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	







WJZⅢ-23A(B)
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary U-shaped foot ring
	WJZH09/10A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	3-lug 2/3-ring
	WJZH02A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Unidirectional extender
	WJZL01A(B)
	Sc/AL/T
	L50～L300，interval2
	1

	
	Bending bar
	WJZL02A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Diagonal brace
	WJZL03A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval2
	1
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	Universal joint
	WJZL08A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	90 ° conversion block
	WJZL11A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	90 ° conversion plate
	WJZL12A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Arc connecting piece
	WJZL14A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	90 ° connecting piece
	WJZL15A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Pitted nut
	WJZL20A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	48

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	48

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	48

	
	earring
	WJZL30A(B)
	Sc/AL/T
	L10～L100，interval2
	3

	
	Quadrangular curved column
	WJZL31A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Adjustable universal hinge
	WJZL32A(B)
	Sc/AL/T
	L10～L200，interval2
	1

	
	Conversion chip
	WJZL33A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Single hole connecting piece
	WJZL34A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Kirschner wire guide block
	WJZL35A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Steering needle base
	WJZL37A(B)
	Sc/AL/T
	L10～L200，interval2
	1

	
	Universal rail connecting piece
	WJZL38A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Ring needle connecting rod
	WJZL39A(B)
	Sc/AL/T
	L10～L300，interval2
	1

	
	Ball bowl gasket
	WJZL40A(B)
	Sc/AL/T
	L5-L400，interval2
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
WJZⅢ-24A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	U-SHAPED FOOT RING
	WJZH04/05A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1
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	Ordinary 1/3 ring
	WJZH08A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Ordinary U-shaped foot ring
	WJZH09/10A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Unidirectional extender
	WJZL01A(B)
	Sc/AL/T
	L50～L300，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	11

	
	Hole slot needle base
	WJZL05 A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Porous connecting piece
	WJZL13A(B)
	Sc/AL/T
	L20～L200，interval1
	2

	
	Arc connecting piece
	WJZL14A(B)
	Sc/AL/T
	L50～L350，interval2
	11

	
	Track connecting piece
	WJZL16A(B)
	Sc/AL/T
	L20～L100，interval2
	1

	
	Threaded column
	WJZL18A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Pitted nut
	WJZL20A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	Hexagonal column
	WJZL21A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	40

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	40

	
	Indenter
	WJZL28A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	control
	WJZL29A(B)
	Sc/AL/T
	L15～L100，interval2
	1

	
	spring
	WJZL27A(B)
	Sc/T
	L15～L100，interval2
	1

	
	earring
	WJZL30A(B)
	Sc/AL/T
	L10～L100，interval2
	3

	
	Adjustable universal hinge
	WJZL32A(B)
	Sc/AL/T
	L10～L200，interval2
	1

	
	Connecting piece
	WJZL36A(B)
	Sc/AL/T
	L40～L200，interval2
	1

	
	Ball bowl gasket
	WJZL40A(B)
	Sc/AL/T
	L5～L400，interval2
	1
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	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
















WJZⅢ-25A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	2

	
	3-lug 2/3-ring
	WJZH02A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	2

	
	Four lug half ring
	WJZH03A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Standard Taylor rod
	WJZW01A(B)
	Sc/AL/T
	L50～260，interval2
	6

	
	Quick mount Taylor bar
	WJZW02A(B)
	Sc/AL/T
	L50～260，interval2
	4

	
	Diagonal brace
	WJZL03A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Offset slot needle base
	WJZL07A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Universal joint
	WJZL08A(B)
	Sc/AL/T
	L5～L400，interval2
	16

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	screw thread Unidirectional joint
	WJZL10A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	Bolt column
	WJZL17A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Quadrangular column
	WJZL19A(B)
	Sc/AL/T
	L10～L150，interval2
	2

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	Ring rod bolt
	WJZL23A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	15

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	42

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	42

	
	earring
	WJZL30A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Ring needle connecting rod
	WJZL39A(B)
	Sc/AL/T
	L10～L300，interval2
	1

	
	Marking card
	WJZL41A(B)
	AL/T
	L5-L400，interval2
	8

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1




26
	

















WJZⅢ-26A(B)
	Six lug full ring
	WJZH01A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	General ring
	WJZH06A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 2/3 ring
	WJZH07A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/3 ring
	WJZH08A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Ordinary 1/2 ring
	WJZH11A(B)
	Sc/AL/Cf/PEEK/T
	R40-R200，interval2
	4

	
	Ordinary U-shaped foot ring
	WJZH09/10A(B)
	Sc/AL/Cf/PEEK/T
	R40～R200，interval2
	1

	
	Unidirectional extender
	WJZL01A(B)
	Sc/AL/T
	L50～L300，interval2
	1

	
	Bending bar
	WJZL02A(B)
	Sc/AL/T
	L50～L350，interval2
	1

	
	Threaded rod
	WJZL04A(B)
	Sc/AL/T
	L50～L350，interval2
	11

	
	Hole slot needle base
	WJZL05A(B)
	Sc/AL/T
	L10～L100，interval2
	4

	
	Half needle base
	WJZL06A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Unidirectional joint
	WJZL09A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	90 ° conversion block
	WJZL11A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	90 ° conversion plate
	WJZL12A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	90 ° connecting piece
	WJZL15A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Pitted bolt
	WJZL20A(B)
	Sc/AL/T
	L5～L400，interval2
	2

	
	bushing
	WJZL22A(B)
	AL/T
	L5～L400，interval2
	6

	
	bolt
	WJZL24A(B)
	Sc/AL/T
	L10～L100，interval2
	20

	
	Washer
	WJZL25A(B)
	Sc/AL/T
	L5～L20,interval1
	53

	
	Nut
	WJZL26A(B)
	Sc/AL/T
	L5～L400，interval2
	53

	
	spring
	WJZL27A(B)
	Sc/T
	L15～L100，interval2
	1

	
	Indenter
	WJZL28A(B)
	Sc/AL/T
	L5～L400，interval2
	1

	
	control
	WJZL29A(B)
	Sc/AL/T
	L15～L100，interval2
	1

	
	Quadrangular curved column
	WJZL31A(B)
	Sc/AL/T
	L10～L150，interval2
	1

	
	Adjustable universal hinge
	WJZL32A(B)
	Sc/AL/T
	L10～L200，interval2
	1
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	Conversion chip
	WJZL33A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Single hole connecting piece
	WJZL34A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Kirschner wire guide block
	WJZL35A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Steering needle base
	WJZL37A(B)
	Sc/AL/T
	L10～L200，interval2
	1

	
	Universal rail connecting piece
	WJZL38A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	
	Connecting sleeve
	WJZL42A(B)
	Sc/AL/T
	L10～L100，interval2
	1

	注：material quality Sc- Stainless steel，AL- aluminium alloy，Cf- carbon fibre，PEEK—Polyetheretherketone， T- titanium alloy
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