Specification & Model：

	Metal Intramedullary Nail
	Specification

	Model
	Product Name
	Diameter D
	Length L

	SNG01-01
	InterZan Femoral Nail (Standard)
	φ9.0、φ9.5、φ10.0、φ10.5、φ11.0、φ11.5、φ12.0、φ12.5
	L180～240

Each 10mm as an increment)

	
	InterZan Femoral Nail (Long)  
	
	L260～420（Left/Right）

(Each 10mm as an increment)

	SNG01-02
	SUFIN Femoral Nail
	φ9.0、φ9.5、φ10.0、φ10.5、φ11.0、φ11.5、φ12.0、φ12.5
	L320～430（Left/Right）

(Each 10mm as an increment)

	SNG01-03
	MASFIN Femoral Nail
	φ9.0、φ9.5、φ10.0、φ10.5、φ11.0、φ11.5、φ12.0、φ12.5
	L320～420（Left/Right）

(Each 10mm as an increment)

	SNG02
	ZAFIN Femoral Nail (Standard)   
	φ9.0、φ9.5、φ10.0、φ10.5、φ11.0、φ11.5、φ12.0、φ12.5
	L180～240(Each 10mm as an increment)

	
	ZAFIN Femoral Nail (Long)  
	
	L260～420（Left/Right）

(Each 10mm as an increment)

	SNG03
	MASRIN Femoral Nail
	φ9.0、φ9.5、φ10.0、φ10.5、φ11.0、φ11.5、φ12.0、φ12.5
	L180～300

(Each 10mm as an increment)

	SNJ01-01
	MASTIN Tibial Nail  
	φ8.0、φ8.5、φ9.0、φ9.5、φ10.0、φ10.5、φ11.0、φ11.5、φ12.0、φ12.5
	L240～360

(Each 10mm as an increment)

	SNWM01～03
	End Cap 1
	Specification
	+0
	+5
	+10
	+15

	
	
	L
	2
	7
	12
	17

	
	End Cap 2
	Specification
	+0
	+5
	+10
	+15

	
	
	L
	2
	7
	12
	17

	
	End Cap 3
	Specification
	+0
	+5
	+10
	+15

	
	
	L
	6
	11
	16
	21

	SNSD01～06
	Locking Bolt 04、

Locking Bolt 06
	φ4.0
	Length 20～95

(Each 1mm as an increment)

	
	
	φ4.5、φ4.9
	Length 25～100

(Each 1mm as an increment)

	
	Locking Bolt 02
	φ4.0
	Length 20～95

(Each 1mm as an increment)

	
	
	φ5.0
	Length 25～100

(Each 1mm as an increment)

	
	Locking Bolt 01、

Locking Bolt 03
	φ6.5、φ7.0、φ10.5、φ11.0
	Length 50～120

(Each 5mm as an increment)


