Annex 1
 Table 1 Type and specification list of Non-absorbable suture anchor               
	Type
	Specification
	REF No.
	Specification

	Type of anchor
	Type of
inserter
	Type of suture
	Anchor
	Suture
	Inserter
	
	

	
	
	
	D±0.1
(mm)
	L+0.1 0
(mm)
	Specification  of suture
	Length of suture L1
(cm)
	L2±2
(mm)
	
	

	SAD
	A
	B
	2.0
	6
	2-0
	90
	172
	NT.Y.MD.0001
	D×L=2.0×6;2-0;L1=90

	SAD
	A
	B
	2.0
	7
	2-0
	90
	169
	
	

	SAB
	A
	L
	2.8
	12
	2
	120
	344
	NT.Y.MD.0109
	D×L=2.8×12;2;L1=120

	SAB
	A
	L
	2.8
	8.8
	2
	120
	341
	
	

	SAA
	A
	L
	3.5
	12
	2
	100
	233
	NT.Y.MD.0845
	D×L=3.5×12;2;L1=100

	SAC
	C
	S
	4.5
	20
	2
	100
	239
	NT.Y.MD.1604
	D×L=4.5×20;2;L1=100

	SAA
	B
	S
	4.5
	15
	2
	100
	230
	
	

	SAA
	B
	S
	5.0
	16
	2
	100
	233
	NT.Y.MD.0998
	D×L=5.0×16;2;L1=100

	SAA
	B
	S
	5.5
	16.2
	2
	100
	230
	
	

	SAC
	C
	S
	5.5
	20
	2
	100
	239
	NT.Y.MD.1698
	D×L=5.5×20;2;L1=100

	SAC
	C
	S
	6.5
	20
	2
	100
	239
	
	












Annex 2
Table 1 Type and specification list of Non-absorbable suture anchor
	Type
	Specification
	Description（D±0.1×L±0.2）mm

	SAA-A-L
	3.5×12
	3.5×12anchor, Type C—w/ one #2 suture(white or blue/white, 100cm) 

	SAA-B-B
	5.0×16
	5.0×16anchor, Type C—w/ one #2 suture(white or blue/white, 100cm)

	NT.SP.T2020NDL
	2.0×6
	2.0×6anchor, Type A—w/ one #2-0 suture (White, 90cm), w/ needle, w/drill 

	NT.SP.T2020DL
	2.0×6
	2.0×6 anchor, Type A—w/ one #2-0 suture (White, 90cm), w/drill

	NT.SP.T1020NDL
	2.0×7
	2.0×7anchor, Type A—w/ one #2-0 suture (White, 90cm), w/ needle, w/drill

	NT.SP.T1020DL
	2.0×7
	2.0×7 anchor, Type A—w/ one #2-0 suture (White, 90cm), w/drill

	NT.SP.T1028N
	2.8×12
	2.8×12anchor, Type B—w/ one #2 suture(white or blue/white, 120cm), w/ needle

	NT.SP.T1028
	2.8×12
	2.8×12anchor, Type B—w/ one #2 suture(white or blue/white, 120cm)

	NT.SP.T2035N
	3.5×12
	3.5×12anchor, Type C—w/ one #2 suture(white or blue/white, 100cm), w/ needle

	NT.SP.T2035
	3.5×12
	3.5×12anchor, Type C—w/ one #2 suture(white or blue/white, 100cm)

	NT.SP.T1035N
	3.5×13
	3.5×13.3anchor, Type E—w/ one #2 suture(white or blue/white, 100cm), w/ needle

	NT.SP.T1035
	3.5×13
	3.5×13.3anchor, Type E—w/ one #2 suture(white or blue/white, 100cm)

	NT.SP.T1045NF
	4.5×20
	4.5×20anchor, Type D—w/two #2 suture(white and blue/white, 100cm), w/needle

	NT.SP.T1045F
	4.5×20
	4.5×20anchor, Type D—w/two #2 suture(white and blue/white, 100cm)

	NT.SP.T2050N
	5.0×16
	5.0×16anchor, Type C—w/two #2 suture(white and blue/white, 100cm), w/needle

	NT.SP.T2050
	5.0×16
	5.0×16anchor, Type C—w/two #2 suture(white and blue/white, 100cm)

	NT.SP.T1050N
	5.4×15.8
	5.4×15.8anchor, Type E—w/two #2 suture(white and blue/white, 100cm), w/needle

	NT.SP.T1050
	5.4×15.8
	5.4×15.8 anchor, Type E—w/two #2 suture(white and blue/white, 100cm)

	NT.SP.T1055NF
	5.5×20
	5.5×20anchor, Type D—w/two #2 suture(white and blue/white, 100cm), w/needle

	NT.SP.T1055F
	5.5×20
	5.5×20anchor, Type D—w/two #2 suture(white and blue/white, 100cm)

	NT.SP.T1065NF
	6.5×20
	6.5×20anchor, Type D—w/two #2 suture(white and blue/white, 100cm), w/needle

	NT.SP.T1065F
	6.5×20
	6.5×20anchor, Type D—w/two #2 suture(white and blue/white, 100cm)

	NT.SP.T1013N
	1.3×3.7
	1.3×3.7anchor, Type F—w/one #2-0 suture(white, 90cm), w/needle

	NT.SP.T1013NDL
	1.3×3.7
	1.3×3.7anchor, Type F—w/one #2-0 suture(white, 90cm), w/needle, w/drill

	NT.SP.T1018N
	1.8×5.4
	1.8×5.4anchor, Type F—w/one #2-0 suture(white, 90cm), w/needle

	NT.SP.T1018NDL
	1.8×5.4
	1.8×5.4anchor, Type F—w/one #2-0 suture(white, 90cm), w/needle, w/drill

	NT.SP.T1024N
	2.4×9.6
	2.4×9.6 anchor, Type F—w/two #2 suture(white, 100cm), w/needle

	NT.SP.T1024NDL
	2.4×9.6
	2.4×9.6anchor, Type F—w/two #2 suture(white, 100cm), w/needle, w/drill

	NT.SP.T1475FT2
	4.75×15
	4.75×15anchor, Type G-w/ one #2 suture(white or blue/white, 100cm), w/ No.2 Tape(white or blue/white)

	NT.SP.T1475FT5
	4.75×15
	4.75×15anchor, Type G-w/ one #2 suture(white or blue/white, 100cm), w/No.5 Tape(white or blue/white)

	NT.SP.T1475F
	4.75×15
	4.75×15anchor, Type G-w/ one #2 suture(white or blue/white, 100cm)）

	NT.SP.T2055FT2
	5.5×15
	5.5×15anchor, Type G-w/ one #2 suture(white or blue/white, 100cm), w/ No.2 Tape(white or blue/white)

	NT.SP.T2055FT5
	5.5×15
	5.5×15anchor, Type G-w/ one #2 suture(white or blue/white, 100cm), w/No.5 Tape(white or blue/white)

	NT.SP.T2055F
	5.5×15
	5.5×15anchor, Type G-w/ one #2 suture(white or blue/white, 100cm)）

	NT.SP.T3055NF
	5.5×20
	5.5×20anchor, Type H-w/two #2 suture(white and blue/white, 100cm), w/needle

	NT.SP.T3055F
	5.5×20
	5.5×20anchor, Type H-w/two #2 suture(white and blue/white, 100cm)








Table 2 Type and specification list of Non-absorbable suture anchor-Drills
	Type
	Specification
（D±0.05）
	Description

	NT.SP.DL001
	1.2mm
	Drill of 2.0mm anchor

	NT.SP.DL002
	1.3mm
	Drill of 1.3mm anchor

	NT.SP.DL003
	2.0mm
	Drill of 1.8mm anchor

	NT.SP.DL004
	2.4mm
	Drill of 2.4mm anchor




Table 3 Type and specification list of Non-absorbable suture anchor-Suture/Tape
	Type
	Specification
	Description

	NT.SP.Tape00
	NO.0
	All-Suture(white or blue/white), Width（W）1.0-1.5mm, Length（L）100±5cm

	NT.SP.Tape01
	NO.1
	All-Suture(white or blue/white), Width（W）1.5-2.0mm, Length（L）100±5cm

	NT.SP.Tape02
	NO.2
	Tape(white or blue/white), Width（W）1.10-1.50mm, Length（L）76±5cm

	NT.SP.Tape03
	NO.3
	All-Suture(white or blue/white), Width（W）2.0-2.5mm, Length（L）100±5cm

	NT.SP.Tape04
	NO.4
	All-Suture(white or blue/white), Width（W）2.5-3.0mm, Length（L）100±5cm

	NT.SP.Tape05
	NO.5
	Tape(white or blue/white), Width（W）1.50-2.00mm, Length（L）100±5cm

	NT.SP.Tape06
	NO.6
	Tape(white or blue/white), Width（W）1.0-1.5mm, Length（L）100±5cm 

	NT.SP.Tape07
	NO.7
	Tape(white or blue/white), Width（W）1.5-2.0mm, Length（L）100±5cm

	NT.SP.Tape08
	NO.8
	Tape(white or blue/white), Width（W）2.0-2.5mm, Length（L）100±5cm

	NT.SP.Tape09
	NO.9
	Tape(white or blue/white), Width（W）2.5-3.0mm, Length（L）100±5cm

	NT.SP.S0020
	NO.2-0
	Suture：White, Length 90cm

	NT.SP.S0002
	NO.2
	Suture：White, Blue/White, Length 100cm

	NT.SP.S0012
	NO.2
	Suture：White, Blue/White, Length 120cm



Annex 3
Table 1 Specification List of All Suture Anchor                        Unit: mm
	Model
	Specification:
W×L(W±3, L±5)
	Description

	NT.SP.AS1301WS
	4×25
	1.3mm all suture anchor with one white 2# suture, type I inserter and O-ring

	NT.SP.AS1301BS
	4×25
	1.3mm all suture anchor with one blue and white 2# suture with type I inserter and O-ring

	NT.SP.AS1301WT
	4×25
	1.3mm all suture anchor with one white type 1 tape, type I inserter and O-ring

	NT.SP.AS1301BT
	4×25
	1.3mm all suture anchor with one blue and white type 1 tape, type I inserter and O-ring

	NT.SP.AS1802S
	5×25
	1.8mm all suture anchor with one white and one blue-white 2# suture, type I inserter and O-ring

	NT.SP.AS1802T
	5×25
	1.8mm all suture anchor with one white and one blue-white type 1 tape, type I inserter and O-ring

	NT.SP.AS2802S
	7×30
	2.8mm all suture anchor with one white and one blue-white 2# suture , type II inserter and O-ring

	NT.SP.AS2802T
	7×30
	2.8mm all suture anchor with one white and one blue-white type 1 tape, type II inserter and O-ring

	NT.SP.AS2802BSWT
	7×30
	2.8mm all suture anchor with one blue and white 2# suture, one white type 2 tape, type II inserter and O-ring

	NT.SP.AS2802WSBT
	7×30
	2.8mm all suture anchor with one white 2# suture, one blue and white type 2 tape, type II inserter and O-ring





Annex 4
Appendix A  Model and Specification List
Model and Specification List of Arthroscopic Approach Cannula
	Model
	Specification
(mm)
	Innner Diameter
Φ±0.5 (mm)
	Length
L±1.5 (mm)
	Washer Thickness
a±0.5(mm)

	NT.SP.G0620
	6×20
	6.0
	20
	5

	NT.SP.G0630
	6×30
	6.0
	30
	5

	NT.SP.G0640
	6×40
	6.0
	40
	5

	NT.SP.G0650
	6×50
	6.0
	50
	5

	NT.SP.G0820
	8×20
	8.0
	20
	5

	NT.SP.G0830
	8×30
	8.0
	30
	5

	NT.SP.G0840
	8×40
	8.0
	40
	5

	NT.SP.G0850
	8×50
	8.0
	50
	5

	NT.SP.G0860
	8×60
	8.0
	60
	5

	NT.SP.G0890
	8×90
	8.0
	90
	5

	NT.SP.G1020
	10×20
	10.0
	20
	5

	NT.SP.G1030
	10×30
	10.0
	30
	5

	NT.SP.G1040
	10×40
	10.0
	40
	5

	NT.SP.G1050
	10×50
	10.0
	50
	5













Annex 5
Appendix A Model and Specification List
Model and Specification List of Graft Preparation System
	Model
	Specifications
	Packaging form
	Components and component specifications

	
	
	
	Suture
	Suture Supporter
	Twister

	NT.SP.K1001
	WB-1000×50L
	1 pcs/box
	#2 Blue and white suture, 1000mm long
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K1002
	WB-1000×40S
	
	#2 Blue and white sutures, 1000mm long
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K1003
	W-1000×50L
	
	#2 White sutures, 1000mm long
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K1004
	W-1000×40S
	
	#2 White sutures, 1000mm long
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K2001
	WB-1000×50L
	2 pcs/box
	#2 Blue and white sutures, 1000mm long
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K2002
	WB-1000×40S
	
	#2 Blue and white sutures, 1000mm long
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K2003
	W-1000×50L
	
	#2 White sutures, 1000mm long
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K2004
	W-1000×40S
	
	#2 White suture, 1000mm long
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K4001
	WB-1000×50L
	4 pcs/box
	#2 Blue and white sutures, 1000mm long
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K4002
	WB-1000×40S
	
	#2 Blue and white sutures, 1000mm long
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K4003
	W-1000×50L
	
	#2 White suture, 1000mm long
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K4004
	W-1000×40S
	
	#2 White sutures, 1000mm long
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K1001-C
	WB-1000×50L-C
	1 pcs/box
	#2 Blue and white sutures, 1000mm long, with suture needle specifications for Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K1002-C
	WB-1000×40S-C
	
	#2 Blue and white sutures, 1000mm long, with suture needle specifications Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K1003-C
	W-1000×50L-C
	
	#2 White sutures, 1000mm long, with suture needle specifications for Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K1004-C
	W-1000×40S-C
	
	#2 White sutures, 1000mm long, with suture needle specifications Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K2001-C
	WB-1000×50L-C
	2 pcs/box
	#2 Blue and white sutures, 1000mm long, with suture needle specifications for Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K2002-C
	WB-1000×40S-C
	
	#2 Blue and white sutures, 1000mm long, with suture needle specifications Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K2003-C
	W-1000×50L-C
	
	#2 White suture, 1000mm long, with suture needle specification Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K2004-C
	W-1000×40S-C
	
	#2 White sutures, 1000mm long, with suture needle specifications Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K4001-C
	WB-1000×50L-C
	4 pcs/box
	#2 Blue and white sutures, 1000mm long, with suture needle specifications for Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K4002-C
	WB-1000×40S-C
	
	#2 Blue and white sutures, 1000mm long, with suture needle specifications Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 40mm long
	33×19

	NT.SP.K4003-C
	W-1000×50L-C
	
	#2 White sutures, 1000mm long, with suture needle specifications for Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 50mm long
	45×19

	NT.SP.K4004-C
	W-1000×40S-C
	
	#2 White sutures, 1000mm long, with suture needle specifications Circle 1/2 arc ·11×20-31
	Flat suture, 1.5mm wide and 40mm long
	33×19













Annex 6
Attachment 2

Model and specification list of Arthroscopic Approach Cannula              Unit: mm
	Model
	Specification
	Inner 
Diameter ɸd
	Outer
 Diameter ɸD
	Length L
	Note

	NT.SP.5075S
	5.0×75
	5.0
	7.7
	75
	Smooth

	NT.SP.6575S
	6.5×75
	6.5
	9.3
	75
	Smooth

	NT.SP.8075S
	8.0×75
	8.0
	10.9
	75
	Smooth

	NT.SP.8575S
	8.5×75
	8.5
	11.1
	75
	Smooth

	NT.SP.5075T
	5.0×75
	5.0
	9.2
	75
	Fully threaded

	NT.SP.6575T
	6.5×75
	6.5
	10.3
	75
	Fully threaded

	NT.SP.8075T
	8.0×75
	8.0
	11.9
	75
	Fully threaded

	NT.SP.8575T
	8.5×75
	8.5
	12.7
	75
	Fully threaded

	NT.SP.5090T
	5.0×90
	5.0
	9.2
	90
	Fully threaded

	NT.SP.6590T
	6.5×90
	6.5
	10.7
	90
	Fully threaded

	NT.SP.8090T
	8.0×90
	8.0
	10.7
	90
	Fully threaded

	NT.SP.8590T
	8.5×90
	8.5
	12.6
	90
	Fully threaded

	NT.SP.8511H
	8.5×110
	8.5
	12.6
	110
	Partially threaded














[bookmark: _GoBack]Annex 7
	Model
	Specification（L*W）
	Color
	Perimeter of applicable parts (cm)
	Applicable systolic blood pressure (mmHg)
	Length of applicable part (cm)

	
	The length of the woven sleeve is L
(not less than 95% of length L)
	Width of woven sleeve W (mm±10)
	
	
	
	

	NT.SP.QZXSZX.S
	400
	75
	Blue
	20~28
	﹤130
	10~40

	NT.SP.QZXSZX.M
	800
	85
	Yellow
	24~40
	﹤130
	20~80

	NT.SP.QZXSZX.L
	800
	95
	Orange
	24~40
	﹤160
	20~80

	NT.SP.QZXSZX.XL
	800
	110
	Black
	24~40
	﹤190
	20~80

	NT.SP.QZXXZX.S
	1000
	85
	Green
	30~55
	﹤130
	40~95

	NT.SP.QZXXZX.M
	1400
	95
	Red
	30~55
	﹤160
	40~110

	NT.SP.QZXXZX.L
	1800
	110
	Pink
	30~55
	﹤190
	40~110

	NT.SP.QZXXZX.XL
	2200
	130
	White
	50~85
	﹤160
	60~120


Model and Specification List of Disposable Exsanguination and Hemostatic Ring

